    [OnInitDialog][MP_MODE_ON] LOCAL_MODE_MP
    [GetCurrentProductIdxFromTxt] currentProduct: 17, currentPidIdx: 2
    [checkProductListExist] Check: FTP_XLS
    [checkProductListExist] => Exist
    [LoadExcelFile] File: .//DATA/List.dll
    [OnInitDialog][MP_MODE_ON] mpModeIsSelected == true
    [SetUpdateProcess] Install driver success
    [SetUpdateProcess] Install driver failed. GetLastError: 0x2
    [OnPaint] STATUS_OF_PNG: -101
    => GUI_SAY_WAITING_FOR_VIDPID
    [DownloadProductListFromFtp] updateMode != SERVER_MODE, checkProductListExist()
    [checkProductListExist] checkProductListExistChecked == true
    [OnPaint] STATUS_OF_PNG: -101
    => GUI_SAY_WAITING_FOR_VIDPID
    [OnPaint] STATUS_OF_PNG: -104
    => GUI_SAY_PLUG (Firmware loaded)
    [OnBnClickedButton2][GUI_SAY_WAITING_FOR_VIDPID] Clicked
    [CheckUpdateDevice] PID-1, Row: 1, Col: 2, VID: 054C, PID: 0CE6
    [OnPaint] STATUS_OF_PNG: -104
    => GUI_SAY_PLUG (Firmware loaded)
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 1, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 1, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 2, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 2, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 2, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 3, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 3, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 3, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 4, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 4, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 4, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 5, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 5, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 5, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 6, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 6, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 6, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 7, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 7, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 7, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 8, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 8, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 8, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 9, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 9, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 9, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 10, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 10, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 10, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 11, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 11, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 11, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 12, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 12, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 12, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 13, Col: 2, VID: 054C, PID: 0CE6
    [OpenDeviceUsb][Success] Vid: 054c, Pid: 0ce6
    Run_WriteFileB(),GetLastError:0x0
    [NewGetVersion][SUCCESS] NewGetVersion Done, newGetVersionReadIdx: 48
    [CheckIcNumFromAPROM] productIdx: 1
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 2
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 3
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 4
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 5
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 6
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 7
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 8
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 9
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 10
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 11
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 12
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 13
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 14
    [CheckIcNumFromAPROM] serverIc: ZPJ211D0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 15
    [CheckIcNumFromAPROM] serverIc: ZPJ210T2, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 16
    [CheckIcNumFromAPROM] serverIc: ZPJ210V0, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: J, deviceIc[2]: V
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [CheckIcNumFromAPROM] productIdx: 17
    [CheckIcNumFromAPROM] serverIc: ZPV01011, strlen(serverIc): 8
    [CheckIcNumFromAPROM] deviceIc: ZPV01010, strlen(deviceIc): 8
    [CheckIcNumOneByOne] serverIc[0]: Z, deviceIc[0]: Z
    [CheckIcNumOneByOne] serverIc[1]: P, deviceIc[1]: P
    [CheckIcNumOneByOne] serverIc[2]: V, deviceIc[2]: V
    [CheckIcNumOneByOne] serverIc[3]: 0, deviceIc[3]: 0
    [CheckIcNumOneByOne] serverIc[4]: 1, deviceIc[4]: 1
    [CheckIcNumOneByOne] serverIc[5]: 0, deviceIc[5]: 0
    [CheckIcNumOneByOne] serverIc[6]: 1, deviceIc[6]: 1
    [CheckIcNumOneByOne] serverIc[7]: 1, deviceIc[7]: 0
    [CheckIcNumOneByOne][ERROR] This device's IC is incorrect!
    [AdjustCurrentProductFromAPROM][ERROR] NOT FOUND: currentProduct
    [CheckUpdateDevice] PID-2, Row: 13, Col: 3, VID: 054C, PID: 1
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 13, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 14, Col: 2, VID: 054C, PID: 09CC
     => Not Found
    [CheckUpdateDevice] PID-2, Row: 14, Col: 3, VID: 054C, PID: 14
     => Not Found
    [CheckUpdateDevice] PID-3, Row: 14, Col: 4, VID: 054C, PID:
     => Skip
    [CheckUpdateDevice] PID-1, Row: 15, Col: 2, VID: 054C, PID: 05C4
     => Not Found
    [CheckUpdateDevice] PID-2, Row: 15, Col: 3, VID: 054C, PID: 15
    [OnBnClickedCancel][Exit]STATUS_OF_PNG: -104